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	GENERAL

	Dimensions & Weight
	74 x 40 mm | 340g

	Usage
	Indoor / Outdoor / Hazardous Locations

	Shackle Dimensions
	Height: 40 mm (standard) 30 mm, 20 mm | Thickness 11 mm

	Build Material
	ZINC Alloy | Bottom Cover: TPE Sealing Cap: Silicon

	ENVIRONMENT

	Temperature
	-40 °C to +85 °C (Operation)

	Relative Humidity (RH)
	0 to 95% (without condensation)

	Ingress Protection
	IP67

	BLE ELECTRONICS

	Power Supply - None
	Lock Powered by a USB Micro rechargeable USB Key Fob – Lithium Battery

	Encryption
	AES 256-bit

	LOGIC

	Accessible Keys
	>2 Million

	Encrypted Audit Trail
	>60,000 Audit Events | >20,000 Cylinders

	COMPATIBILITY

	Keys
	All Key BLE Types / Rechargeable USB BLE 4.0 Lithium – via USB Mini C

	CERTIFICATIONS

	CE / NIST / BLE / NEMA TS-2

	WARRANTY

	Warranty
	5 years
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BlueKey™ 
Rugged, Military Grade, 
ZINC Alloy
, Encrypted, Bluetooth Low Energy (BLE)
,
 
High 
Security Padlock. 
No wires, No Batteries 
& No Maintenance.
 
America’s #1 Security Padlock for use indoors or outdoors. 
Waterproof and Dustproof – IP65 Ingress Protection
 
 
5 Year Warranty – NIST Compliant 
– Patent 
Pending
)[image: ]
image4.jpeg




image1.png




image2.png




image3.jpeg
Diamond Shape




