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DY-H8080XR
DYMEC – Hardened, Industrial 8 port Gigabit Flat PoE Switch,
8 x 10/100/1000 TX, 30 Watt PSE, 2KV Surge Immunity / Isolation
Supports power 1, power 2, and power din (for external power adapter),
Input Voltage: 48 ~ 56 Volts DC, Operating Temperature: -40°C to +75°C 


Din rail mount

Wall mount 
Cabinet
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Introduction

This Industrial 8 port POE switch is designed for IP surveillance, traffic monitoring, industrial applications and for a broad range of other applications. The unique flat design is perfect for space-limited environments, such as a shallow cabinet or a small enclosure. It is equipped with 8 x 30W PSE ports, and can deliver up to 200 Watts of power to your PD devices. It can be used as a stand-alone device for buses, trucks, and other vehicles for surveillance purposes. It has been rigorously tested for your security, transportation and telco applications.





Specifications
	IEEE Standard
	IEEE 802.3 10Base-T Ethernet
IEEE 802.3u 100Base-TX Fast Ethernet
IEEE 802.3ab 1000Base-T Gigabit Ethernet
IEEE 802.3x Flow Control and Back Pressure,
IEEE 802.3af for POE
IEEE 802.3at for POE+

	
	

	Switch Architecture
	Back-plane (Switching Fabric): 17Gbps 

	Data Processing 
	Store and Forward

	Flow Control
	IEEE 802.3x Flow Control and Back Pressure 

	Jumbo Frame
	9KB

	MAC address Table Size
	4K

	Packet Buffer Size
	1Mbits

	Network Connector 
	8 x RJ-45 10/100/1000BaseT(X) auto negotiation, 
Auto MDI/MDI-X function, Full/Half duplex  
8 x Gigabit POE+ 802.3at/af PSE port, 30 Watts per port            

	Network Cable
	UTP/STP above Cat.5e Cable

	
	EIA/TIA-568 10-ohm (100m)

	Protocol
	CSMA/CD

	LED
	PW1 (Green): ON－Power 1 is detected
PW2 (Green): ON－Power 2 is detected
PW3 (Green): ON－Power 3 is detected for Power DIN
RLY (Amber): ON－Connect only PW1 or PW2
                          OFF－Both PW1 and PW2 are 
                                     connected

	
	TX/RJ-45 port:
LNK (Link/Active) (Green): ON－TX port is detected
Flashing－TX data is 
                            transmitting/receiving
POE (Amber): ON－PD is detected and PSE is activated
  OFF－PD is not detected

	Reserve polarity protection
	Yes

	Overload current protection
	Yes

	Power Supply
	Redundant Dual DC 48 ~ 56 Volt Power Inputs

	Power Consumption
	5.76 Watts @ 48 Volts DC full load, Without POE






	Alarm Relay Contact
	Relay outputs - current carrying capacity of 1 AMP @ 24 Volts DC,  
Relay in open circuit mode when 2 powers are connected. in short circuit mode when only one power supply is connected

	POE power
	POE power per port 30 Watts.
Maximum total power 240 Watts with 56VDC input, Supports IEEE802.3af/at

	Removable Terminal Block
	Provides 2 Redundant power inputs, Alarm relay contact ,6 Pin
Wire range: 0.34mm^2 to 2.5mm^2
Solid wire (AWG):12-24/14-22
Stranded wire(AWG): 12-24/14-22
Torque:5lb-In/0.5Nm/0.56Nm
Wire Strip length: 7-8mm

	Operating Temperature
	-40°C to +85°C 

	Operating Humidity
	5% to 95% (Non-condensing)

	Storage Temperature
	-40°C to 85°C

	MTBF (mean time between failure)
	>525,000 hours ( MIL-HDBK-217F) at 25°C

	Housing 
	Military Grade with Aluminum, IP30 Protection

	Case Dimension 
	150 x 145 x 26.7 mm (L x W x D)
198 x 145 x 26.7 mm (L x W x D) (with brackets)

	Weight
	0.75kg (with brackets)

	Installation
	DIN Rail Mount or Wall Mount
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	Safety
	LVD(EN60950-1)

	EMC
	CE, FCC, EN 55032/24, NEMA TS-2

	EMI
	CISPR 32, FCC Part 15B Class A

	EMS  
	IEC 61000-4-2 ESD: Contact: 6KV; Air: 8KV
IEC 61000-4-4 EFT: Power: 2KV; Signal: 2KV
IEC 61000-4-5 Surge: Power: 2KV; Signal: 2KV

	Vibration
	EN 60068-2-6

	Shock
	EN 60068-2-27

	Free Fall
	EN 60068-2-32





Housing Dimensions (mm)
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