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Safety
[bookmark: _Hlk514744827][bookmark: _Hlk514744826]UL 60950-1
DY-HI8011-9bt - Hardened 90-Watt. Gigabit, IEEE 802.3bt, POE Injector
1 x 95 Watt Gigabit TX PSE + 1 x Gigabit TX, 48-56 Volts DC input voltage, 
Operating temp.: -40°C to +75°C


Features: 
[image: Macintosh HD:Users:michaelho:Dropbox:michael:PIC:141105:HI8011-30W small.png]
· Safety UL60950-1 Certified
· Rugged Military Grade Aluminum Housing
· [image: Macintosh HD:Users:michaelho:Documents:PRIMMCON:product:Industrial POE sereis:H8042C:photo:DINR.jpg]Deliver ultrahigh power up to 95Watts
· Supports Redundant Power Inputs
· Working in extreme environment -40 to +85°C





DY-HI8011-90bt

Overview

This ultrahigh power hardened Gigabit POE Injector is equipped with 1 x 90-Watt Gigabit PSE port to power up to 90 Watts PD devices. Used for camera, WiFi AP, or LoRa applications. This unit was made especially for IP surveillance, traffic monitoring, outdoor cameras and for a broad range of power applications. It can tolerate -40°C to +75°C in harsh environments.



Specifications
	IEEE Standard
	IEEE 802.3 10Base-T Ethernet
IEEE 802.3u 100Base-TX Fast Ethernet
IEEE 802.3ab 1000Base-T Gigabit Ethernet
IEEE 802.3 af/at/bt 

	
	

	Network Connector
	1xRJ-45 10/100/1000BaseT(X) Data
1xRJ-45 10/100/1000BaseT(X) Data with POE Output Power

	Network Cable
	UTP/STP Cat.5e or above  Cable

	
	EIA/TIA-568 10-ohm (100m)

	Protocol
	CSMA/CD

	LED
	PW1 (Green): ON－Power is detected
PW2 (Green): ON－Power is detected
Mode A (Green): For End-Span PoE power 1,2,3,6
Mode B (Green): Reserved

	POE Pin Assignment
	Pin 1 (V-), 2 (V-), 3 (V+), 6 (V+)
Pin 4 (V+), 5 (V+), 7 (V-), 8 (V-)

	Reverse polarity protection
	Present 

	Overload current protection
	Present

	Power Supply
	2 Redundant input power sources 
48V-57V VDC Power Input 

	Power Consumption
	1 Watt @48 VDC Without POE

	POE power
	Maximum POE power 95watts at 56VDC input

	Removable Terminal Block
	Provide 4 pin terminal block
Wire range: 0.34mm^2 to 2.5mm^2
Solid wire (AWG):12-24/14-22
Stranded wire(AWG): 12-24/14-22
Torque:5lb-In/0.5Nm/0.56Nm
Wire Strip length: 7-8mm

	Operating Temperature
	-40°C to 85°C

	Operating Humidity
	5% to 95% (Non-condensing)

	Storage Temperature
	-40°C to 75°C

	MTBF (mean time between failure)
	>5000,000 hours ( MIL-HDBK-217F) at 25°C

	Housing 
	Rugged Aluminum, IP30 Protection

	Case Dimension (L X W X D)mm
	103.5 x 32 x 81.5 mm (L x W x D)

	Installation mounting 
	DIN Rail and Wall Mount options included  









	Certifications:

	Safety
	UL 60950-1

	Safety
	IEC EN60950-1

	EMC/EMS  
	CE, FCC, VCCI

	EN 60068-2-6
	Vibration

	EN 60068-2-27
	Shock

	EN 60068-2-32
	Free Fall
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