**KY-3170™EM4 / DYMEC 3170™ Series**

**6x4 Port, Managed, Gigabit, Temperature Hardened, ITS, Industrial, Input File, Ethernet Switch – Low Power / NSA Endpoint Certified with ERPsv2**



|  |  |
| --- | --- |
|  | * **6x Gigabit Ethernet ports** * **4x 1000 Mbps SFP Slot (Mini Gbic) / ERPS Multi Ring** * **NSA Network Endpoint Guideline Certified for Console Port Shutdown and Chassis Full Security (Patent Pending)** * Built for harsh environments and wide temperature range applications / Edge Computing * RSTP, MSTP, ERPS, LACP for Network Redundancy * QoS CoS/DSCP to increase determinism * Input File / Low Power Industrial Ethernet Switch * Supports IGMP Snooping v1/v2/v3, up to 1024 groups * DHCP Relay Option 82 IP address assignment * SNMP v1/v2c/v3 for network management * Supports Storm Protection / Broadcast Control * USB storage for configuration-free replacement * Supports industrial automation protocols Ethernet/IP & Modbus TCP * Secure File Transfer Protocol (SFTP) & Trivial File Transfer Protocol (TFTP)   A close up of a sign  Description generated with very high confidenceA close up of a sign  Description automatically generated |
|  |
|  | |
| **Specifications** | |

|  |  |
| --- | --- |
| **Technology** | |
| **Standards** | IEEE 802.3 10BaseT  IEEE 802.3u 100BaseTX  IEEE 802.3ab 1000BaseT  IEEE 802.3z 1000BaseX  IEEE 802.3x Flow Control  IEEE 802.3ad/802.1AX LACP  IEEE 802.1D Spanning Tree Protocol  IEEE 802.1w Rapid STP  IEEE 802.1s Multiple STP  ITU-T G.8032 / Y.1344 ERPS  IEEE 802.1Q VLAN Tagging  IEEE 802.1ad Stacked VLANs  IEEE 802.1p Class of Service  IEEE 802.1X Network Authentication  IEEE 802.1AB LLDP |
| **Processing Type** | Store and Forward |
| **Switch Properties** | |
| **Priority Queues** | 8 Queues |
| **Jumbo Frame** | 16000bytes |
| **MAC Table Size** | 16K |
| **VLAN Table Size** | 4094 |
| **IGMP Group** | 1023 |
| **Packet Buffer** | 12Mbits |
| **Software Features** | |
| **Network Redundancy** | RSTP, MSTP, G.8032 ERPSv2, Port Trunking with LACP |
| **Security** | 802.1X, RADIUS, TACACS+, SSL, SSH, ACL / Security ACL Package |
| **Management** | IPv4, IPv6, Web, Telnet, Serial Console, CLI, SFTP, SNMP v1/v2c/v3, uPnP |
| **Diagnostics** | RMON, SNMP Inform/Trap, Syslog, SMTP, Port Mirroring, LLDP, DDMI, Cable Diagnostic\* |
| **Configuration** | DHCP Server/Client, Relay Option 82, TFTP, SFTP, USB |
| **Filter** | 802.1Q VLAN, Q-in-Q, IGMP Snooping v1/v2/v3, IGMP Querier, Independent Vlan Learning |
| **Time Sync.** | NTP |
| **QoS** | CoS, DSCP, WRR/SPQ Queuing, Storm Protection, Broadcast Control |
| **Industrial Profiles** | Ethernet/IP, Modbus TCP |
| **Switch Interfaces** | |
| **RJ45 Port** | 6 x 10/100/1000T(x), auto negotiation speed duplex mode, auto MDI/MDI-X |
| **Fiber Port** | 4 x 1000 Mbps SFP Slots |
| **LED Indicators** | **Per unit:** PWR1, Fault, Ring Master, Ring State  **Ports:** Link/Active with highest speed(Green), low speed(Amber) |
| **Button** | Multiple functions reset button |
| **Serial Console** | 1 x RS232 in RJ45 connector with console cable, 115.2Kbps, 8N1 |
| **Storage** | 1 x USB 2.0 storage for firmware update, configuration backup, restore, boot up and syslog |
| **Power Requirements** | |
| **Operation Voltage** | 12 ~ 24 ~48 Volts DC |
| **Connection** | PCB Golden Finger |
| **Power Consumption** | [0.58A@24](mailto:0.58A@24) Volts DC |
| **Protection** | Overload Current Protected, Reverse Polarity Protected |
| **Mechanical Construction** | |
| **Enclosure** | Metal / Military - Structural Grade |
| **Protection Class** | IP30 |
| **Dimensions** | 58 x 114 x 205 mm (W x H x D) |
| **Weight** | 0.87 kg |
| **Mounting** | Input File / Rack Mount with Rail Slots |
| **Environmental Limits** | |
| **Operating Temperature** | -40°C ~ 80°C (-40°F ~ 176°F) |
| **Storage Temperature** | -40°C ~ 85°C (40°F ~ 185°F) |
| **Ambient Relative Humidity** | 5 to 95%, (Non-Condensing) |
| **Regulatory Approvals** | |
| **Altitude – GB4943.1-2011** | 0 ~ 5000 Meters |
| **EMI** | FCC Part 15 Subpart B Class A  CE EN 55032 Class A |
| **EMS** | IEC61000-4-2 (ESD)  IEC61000-4-3 (RS)  IEC61000-4-4 (EFT)  IEC61000-4-5 (Surge)  IEC61000-4-6 (CS)  IEC61000-4-8 (Magnetic Field) |
| **Free Fall** | IEC60068-2-32 |
| **Shock** | IEC60068-2-27 |
| **Vibration** | IEC60068-2-6 |
| **Green** | RoHS Compliant |
| **Certifications** | UL 60950-1/62368  61000-6-2 / FCC / NEMA TS-2  61000-6-4 / ITUT / IEEE |
| **MTBF**  **MIL-HDBK-217**  **IEC 62380** | >177,000 hours |
| **Warranty**  **TAA Compliant** | 5 Years / Limited Lifetime  Certified TAA Compliant |


|  |
| --- |
| **Note from DYMEC Development**  **In a continuing effort of improvement and updated technology, product specifications are subject to change without notice.** |
|  |
| **Dimensions (unit = mm)** |
|  |

**DYMEC 3170 Supports: 2 & 4 Wire LONG RANGE ETHERNET / VDSL2 SFP Modem**

With long reach coverage, high noise immunity, and compact board size, **DYMEC KY-Pro-180-CRD Ruggedized** SFP modem is an ideal upgrade for your Enterprise or Industry applications. Used in Pairs.

**VDSL2 – Long Range Ethernet Application (KY-Pro-180-CRD)**

|  |  |
| --- | --- |
| MECHANICAL DIMENSIONS | Copper Ring Fiber Ring Indu |

**DYMEC KY-SFP-T**

Copper SFP Transceiver – Used to Add Additional RJ-45 Copper Ports to your KY-3170 Series Switch

Easy to Install & Configure – GUI Selectable

|  |  |
| --- | --- |
|  | |
| **Ordering Information** | |
| **KY-3170™EM4**  **DYMEC 3170™ Series** | **6+4 Port, Industrial, Managed, Gigabit Ethernet ITS Switch**  **- 6 x 10/100/1000T(x) + 4 x 1000 SFP Slots / ERPS**  **- Operating Temperature: -40°C ~ 80°C (-40°F ~ 176°F)**  **NSA Guideline Certified for Console Port Shutdown and Chassis Full Security** |

|  |  |
| --- | --- |
| **KY-3170™EM4/2**  **DYMEC 3170™ Series** | 6+4 Port, Industrial, Managed, Gigabit Ethernet ITS Switch (Configured 8 Copper RJ45 Ports)  - 6 x 10/100/1000T(x) + 2 x 10/100/1000 Copper SFP + 2 x 1000 SFP Slot / ERPS  - Operating Temperature: -40°C ~ 80°C (-40°F ~ 176°F)  **NSA Guideline Certified for Console Port Shutdown and Chassis Full Security** |

**DYMEC – Temperature Hardened, American Made, Ruggedized, NSA Certified Endpoint, Industrial Ethernet Switches / Routers for SCADA, ITS, Transportation, Automation, Power Utilities, Edge Computing, AI and Industrial Control Systems****.** **Made in USA. Cyber-Secure, TAA Compliant. Uses SFP’s / BiDi SFP’s / Mini Gbic** **& VDSL2 Industrial SFP for Long Range Ethernet.**

**A close up of a sign

Description automatically generated**A close up of a sign

Description generated with very high confidence

