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Rugged, Military Grade, 
ZINC ALLOY & 304 Stainless Steel
, Encrypted, Bluetooth Low Energy (BLE)
,
 
***
High 
Security 
Traffic Enclosure Lock
. 
Exact Replacement!
 Precision Cast – Lightweight & Stronger
No wires, No Batteries 
& No Maintenance.
 
America’s #1
 Traffic Enclosure Lock
. 
Waterproof and Dustproof – IP65 Ingress Protection
. Full Audit Trail
 
5 Year Warranty – NIST Compliant 
– Patent Pending
)BW-BTE207 Traffic Enclosure Lock
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	GENERAL

	Dimensions & Weight
	130 x 80 x 90 mm | 340g / Precision Cast

	Usage
	Indoor / Outdoor / Hazardous Locations

	Exact Replacement
	Yes – Bolt for Bolt Interchangeable. No wiring, No drilling or door modifications

	Build Material
	304 Stainless Steel | Bottom Cover: TPE Sealing Cap: Silicon

	ENVIRONMENT

	Temperature
	-40 °C to +85 °C (Operation)

	Relative Humidity (RH)
	0 to 95% (without condensation)

	Ingress Protection
	IP65

	ELECTRONICS

	Power Supply - None
	Lock Powered by a USB Micro rechargeable USB Key Fob – Lithium Battery

	Encryption
	AES 256-bit

	LOGIC

	Accessible Keys
	>2 Million

	Encrypted Audit Trail
	>60,000 Audit Events | >20,000 Cylinders

	COMPATIBILITY

	Keys
	All Key Types / Rechargeable USB BLE 4

	CERTIFICATIONS

	CE / NIST / BLE / NEMA TS-2

	WARRANTY

	Warranty
	3 years
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